#AP6234_NVRAM_V1.2_20140820_WIN8.1
manfid=0x2d0
prodid=0x0653
vendid=0x14e4
devid=0x4386
boardtype=0x0653
boardrev=0x1203
boardnum=22
macaddr=00:90:4c:c5:12:38
sromrev=3
#boardflags: 
# bit 19 3tswitch:   2.4GHz FEM: SP3T switch share with BT
# bit 16	 nopa:   no external pa
#            keep original 0x200
boardflags=0x0090201
xtalfreq=37400
nocrc=1
ag0=255
aa2g=1
ccode=CN
pa0itssit=0x20
#PA parameters for 2.4GHz
#pa0b0=6957 default
pa0b0=6727 
pa0b1=-858
pa0b2=-178
tssifloor2g=69
# rssi params for 2.4GHz
rssismf2g=0xf
rssismc2g=0x8
rssisav2g=0x1
cckPwrOffset=3

# rssi params for 5GHz
rssismf5g=0xf
rssismc5g=0x7
#rssisav5g=0x1
rssisav5g=0x3

#PA parameters for lower a-band
#pa1lob0=5659 default
pa1lob0=5859
#pa1lob0=5659
pa1lob1=-693
pa1lob2=-178
tssifloor5gl=77

#PA parameters for midband
pa1b0=5372 
#pa1b0=5172
pa1b1=-671
pa1b2=-212
tssifloor5gm=77

#PA paramasdeters for high band
#pa1hib0=5320 default
pa1hib0=5620
#pa1hib1=-963
pa1hib1=-663
pa1hib2=-179
tssifloor5gh=74

rxpo5g=0
maxp2ga0=72
#  19.5dBm max; 18dBm target
#Per rate power back-offs for g band, in .5 dB steps. Set it once you have the right numbers.
cck2gpo=0xaaaa
ofdm2gpo=0x77777777
# R54 16dBm; R48 17dBm; others 18dBm
mcs2gpo0=0xdddd
# M0~ M4 17dBm
mcs2gpo1=0xdddd
# M5M6 15dBm; M7 14.5dBm
#max power for 5G
maxp5ga0=68
# 16dBm target; 17.5dBm Max 
maxp5gla0=68
maxp5gha0=68
#Per rate power back-offs for a band, in .5 dB steps. Set it once you have the right numbers.
ofdm5gpo=0x22222222
# R54 13.5dBm
ofdm5glpo=0x22222222
ofdm5ghpo=0x22222222
mcs5gpo0=0x8888
# M0~M4 16dBm (1dB higher than ofdm)
mcs5gpo1=0x4444
# M5M6 13.5dBm; M7 12dBm
mcs5glpo0=0x4444
mcs5glpo1=0x4444
mcs5ghpo0=0x4444
mcs5ghpo1=0x4444
# Parameters for DAC2x mode and ALPF bypass
# RF SW Truth Table: ctrl0 for BT_TX; ctrl1 or 5G Tx; ctrl2 for 5G Rx; Ctrl3 for 2G Tx; Ctrl4 for 2G Rx
swctrlmap_2g=0x00080008,0x00100010,0x00080008,0x011010,0x11f
swctrlmap_5g=0x00040004,0x00020002,0x00040004,0x011010,0x2fe
gain=32
triso2g=8
triso5g=8
#tx parameters
loflag=0
iqlocalidx5g=40
dlocalidx5g=70
iqcalidx5g=50
lpbckmode5g=1 
txiqlopapu5g=0
txiqlopapu2g=0
dlorange_lowlimit=5
txalpfbyp=1
txalpfpu=1
dacrate2xen=1
papden2g=1
papden5g=1
#rx parameters
gain_settle_dly_2g=4
gain_settle_dly_5g=4
noise_cal_po_2g=-1
noise_cal_po_40_2g=-1
noise_cal_high_gain_2g=73
noise_cal_nf_substract_val_2g=346
noise_cal_po_5g=-1
noise_cal_po_40_5g=-1
noise_cal_high_gain_5g=73
noise_cal_nf_substract_val_5g=346
cckpapden=0
# Enable OOB interrupt: level trigger
#muxenab=0x10
# Out-of-band GPIO wakeup
sd_gpout=4
sd_gpval=1
sd_gpdc=0
btc_flags=71
btc_params8=15000
btc_params22=8000
btc_params83=9000
btc_params84=4500
rssicorrnorm=15
